{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["配置清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"配置清单","index":0,"n_rows":11,"n_cols":7,"rows_kept":11,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["幼儿园采购盥洗室等视频监控系统清单"]
["序号","名称","型号","功能参数","数量","单位","备注"]
[1,"400万红外定焦海螺网络摄像机","DH-IPC-HDW3430T-A","1.传感器类型：1/3英寸CMOS；\n2.像素：400万；最大分辨率：2560×1440；\n3.最低照度：0.01lux（彩色模式）；0.001lux（黑白模式）；0lux（补光灯开启）；\n4.最大补光距离：50m（红外）；补光灯：2颗（红外灯）；\n5.镜头类型：定焦；镜头焦距：2.8-3.6mm（可选）；镜头光圈：F2.0；视场角：水平：76°；垂直：40°；对角：92°；\n6.智能编码：H.264:支持；H.265:支持；宽动态：支持；内置MIC：支持；\n7.报警事件：网络断开；IP冲突；非法访问；动态检测；视频遮挡；音频异常侦测；安全异常；\n8.供电方式：DC12V/PoE；\n9.防护等级：IP67。",13,"台","2.8镜头"]
[2,"400万红外枪型网络摄像机","DH-IPC-HFW3430M-A-I1","1.传感器类型：1/3英寸CMOS；像素：400万；最大分辨率：2560×1440；\n2.最低照度：0.01lux（彩色模式）；0.001lux（黑白模式）；0lux（补光灯开启）；\n3.最大补光距离：50m（红外）；补光灯：1颗（红外灯）；\n4.镜头类型：定焦；镜头：3.6mm/6mm/8mm可选；\n4.镜头光圈：F2.0；视场角：水平：48°；垂直：28°；对角：56°；\n5.智能编码：H.264:支持；H.265:支持；宽动态：支持；内置MIC：支持；\n6.报警事件：网络断开；IP冲突；非法访问；动态检测；视频遮挡；音频异常侦测；安全异常；\n7.供电方式：DC12V/PoE；\n8.防护等级：IP67。",1,"台"]
[3,"8口POE交换机（千兆）","RG-ES110GDS-P-E","1.千兆以太网交换机，具有8口10/100/1000Mbps自适应电口交换机；\n2.背板交换容量20Gbps，包转发率14.88Mpps；MAC地址表4K；\n3.支持PoE/PoE+，PoE功率120W，固化2个SFP千兆光口。",3,"个"]
[4,"存储硬盘（10T）","ST10000NM017B","1.企业级存储专用硬盘，需与原存储设备兼容适用；\n2.容量：10T；转速：7200RPM；缓存容量：256M；接口：SATA3.0。",3,"个","满足三个月摄像头存储"]
[5,"非屏蔽六类双绞线","HD1604004","1.性能符合ANSI/TIA-568-C.2-2009、GB/T 50312-2016、IEC 61156-5六类标准；\n2.采用中心PE十字骨架，精确的不同线对扭绞节距搭配和平衡设计，减小了近端串扰损耗（NEXT）。\n3.适用于语音、数据、图像、多媒体等信息传输。",3,"箱"]
[6,"集中供电器","小耳朵，STD-WAX120-12L","1.电压范围：200-240V；效率：>85%；交流电流：25AMax；\n2.直流电压：12V；额定电流：10A；额定功率：120W；\n3.工作温度：-20℃ — +45℃；工作湿度：20%-90% RH，无冷凝。",1,"个"]
[7,"配管","国标、PVC20","国标，∅20",350,"米","包括连接件材料"]
[8,"电源线","国标、RVV-3*1.5","国标、RVV-3*1.5",50,"米"]
[9,"实施及辅材","现场实施","设备安装、调试，及现场配套实施所需扎带、跳线、标签等辅材。",1,"项","含吊顶拆卸和安装（不得影响日常教学工作，要求只能周末期间施工）"]